;; Jz4740_usb.inf

;; *********  PLEASE READ ***********
;; The wizard cannot create exact INF files for all buses and device types.
;; You may have to make changes to this file in order to get your device to
;; install. In particular, hardware IDs and logical configurations require
;; intervention.
;;
;; The Windows DDK documentation contains an excellent INF reference.

;--------- Version Section ---------------------------------------------------

[Version]
Signature="$Windows 95$"
Class=NewDeviceClass
ClassGUID={ff646f80-8def-11d2-9449-00105a075f6b}
Provider=%ProviderName%
DriverVer=09/14/2008,1.4.0000.0


;--------- SourceDiskNames and SourceDiskFiles Section -----------------------

; These sections identify source disks and files for installation.  They are
; shown here as an example, but commented out.

;[SourceDisksNames]
;1 = "Install Disk",Disk1,,

;[SourceDisksFiles]
;jz4740_usb.sys = 1,,

;--------- ClassInstall/ClassInstall32 Section -------------------------------

; Not necessary if using a standard class

; 9X Style
[ClassInstall]
Addreg=Class_AddReg

; NT Style
[ClassInstall32]
Addreg=Class_AddReg

[Class_AddReg]
HKR,,,,%DeviceClassName%
HKR,,Icon,,"-18"

;--------- DestinationDirs Section -------------------------------------------

[DestinationDirs]
Jz4740_usb_Files_Driver = 10,System32\Drivers

;--------- Manufacturer and Models Sections ----------------------------------

[Manufacturer]
%MfgName%=Mfg0

[Mfg0]
%DeviceDesc%=Jz4740_usb_DDI, USB\VID_601a&PID_4740
%DeviceDesc%=Jz4740_usb_DDI, USB\VID_601a&PID_4750

;---------- DDInstall Sections -----------------------------------------------
; --------- Windows 9X -----------------

; Experimentation has shown that DDInstall root names greater than 19 characters
; cause problems in Windows 98

[Jz4740_usb_DDI]
CopyFiles=Jz4740_usb_Files_Driver
AddReg=Jz4740_usb_9X_AddReg

[Jz4740_usb_9X_AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,jz4740_usb.sys
HKR, "Parameters", "BreakOnEntry", 0x00010001, 0
; --------- Windows NT -----------------

[Jz4740_usb_DDI.NT]
CopyFiles=Jz4740_usb_Files_Driver
AddReg=Jz4740_usb_NT_AddReg

[Jz4740_usb_DDI.NT.Services]
Addservice = Jz4740_usb, 0x00000002, Jz4740_usb_AddService

[Jz4740_usb_AddService]
DisplayName    = %SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\Usb_Boot_Driver.sys

[Jz4740_usb_NT_AddReg]
HKLM, "System\CurrentControlSet\Services\Jz4740_usb\Parameters",\
	"BreakOnEntry", 0x00010001, 0



; --------- Files (common) -------------

[Jz4740_usb_Files_Driver]
Usb_Boot_Driver.sys

;--------- Strings Section ---------------------------------------------------

[Strings]
ProviderName="Ingenic Semiconductor"
MfgName="Ingenic Semiconductor"
DeviceDesc="Usb Boot Device"
DeviceClassName="Ingenic Usb Boot Class"
SvcDesc="version 1.4b"